**Liverani Flexible Impeller Pump EP Model Numbers.**

**EP MINI ¾” –** 0.37Kw, 1-3 phase 230-400v, Single speed operation. 900 rpm. Max Flow 900 L/h, max head 18M.

**EP MINI ¾” –** 0.56Kw, 1-3 phase 230-400v, Single speed operation. 1400 rpm. Max Flow 1440 L/h, max head 30M.

**EP MINI ¾” –** 0.3Kw, direct current 12-24v, Single speed operation. 1400 rpm. Max Flow 1440 L/h, max head 30M.

**EP MIDEX 1” ¼ -** 0.56Kw, 1-3 phase 230-400v, Single speed operation. 900 rpm. Max Flow 3480 L/h, max head 24M.

**EP MIDEX 1” ¼ -** 0.75Kw, 1-3 phase 230-400v, Single speed operation. 1400 rpm. Max Flow 5160 L/h, max head 27M.

**EP MIDEX 1” ¼ -** 0.56Kw, three phase 230-400v, 2 speed operation. 1400 rpm. Max Flow 5160 L/h, max head 27M.

**EP MIDEX 1” ¼ -** 0.37Kw, three phase 230-400v, 2 speed operation. 700 rpm. Max Flow 2600 L/h, max head 18M.

**EP MIDEX 1” ¼ -** 0.5Kw, direct current 24v, Single speed operation. 900 rpm. Max Flow 3480 L/h, max head 24M.

**EP MINOR 40 –** 1.5Kw, 1-3 phase 230-400v, Single speed operation. 900 rpm. Max Flow 6200 L/h, max head 24M.

**EP MINOR 40 -** 1.5Kw, three phase 230-400v, Single speed operation. 1400 rpm. Max Flow 9000 L/h, max head 27M.

**EP MINOR 40 -** 1.87Kw, three phase 230-400v, 2 speed operation. 1400 rpm. Max Flow 9000 L/h, max head 27M.

**EP MINOR 40 -** 1.35Kw, three phase 230-400v, 2 speed operation. 900 rpm. Max Flow 6200 L/h, max head 24M.

**EP MAJOR 60 –** 1.25Kw, three phase 230-400v, Single speed operation. 470 rpm. Max Flow 10500 L/h, max head 12M.

**EP MAJOR 60 -** 1.5Kw, three phase 230-400v, Single speed operation. 700 rpm. Max Flow 15000 L/h, max head 16M.

**EP MAJOR 60 -** 1.87Kw, three phase 230-400v, Single speed operation. 900 rpm. Max Flow 19560 L/h, max head 16M.

**EP MAXI 80 –** 3.3Kw, three phase 230-400v, Single speed operation. 470 rpm. Max Flow 34200 L/h, max head 16M.

**EP MAXI 80 –** 3.5Kw, three phase 230-400v, Single speed operation. 600 rpm. Max Flow 41400 L/h, max head 16M.