**Liverani Flexible Impeller Pump GR Model Numbers.**

**GR MINOR 40 –** 1.5Kw, 1-3 phase 230-400v, single speed operation. 300 rpm. Max Flow 2150 L/h, max head 16M.

**GR MINOR 40 –** 1.5Kw, 1-3 phase 230-400v, single speed operation. 470 rpm. Max Flow 3300 L/h, max head 18M.

**GR MINOR 40 -** 1.5Kw, 1-3 phase 230-400v, single speed operation. 700 rpm. Max Flow 4700 L/h, max head 20M.

**GR MINOR 40 -** 1.6Kw, 3 phase 230-400v, 2 speed operation. 470 rpm. Max Flow 3300 L/h, max head 18M.

**GR MINOR 40 –** 0.9Kw, 3 phase 230-400v, 2 speed operation. 235 rpm. Max Flow 1600 L/h, max head 12M.

**GR MINOR 40 –** 2.2Kw, 3 phase 230-400v, 2 speed operation. 700 rpm. Max Flow 4700 L/h, max head 20M.

**GR MINOR 40 –** 1.5Kw, 3 phase 230-400v, 2 speed operation. 350 rpm. Max Flow 2500 L/h, max head 16M.

**GR MAJOR 60 –** 1.5Kw, 1-3 phase 230-400v, single speed operation. 470 rpm. Max Flow 10500 L/h, max head 12M.

**GR MAJOR 60 –** 1.86Kw, 3 phase 230-400v, single speed operation. 700 rpm. Max Flow 15000 L/h, max head 16M.

**GR MAJOR 60 –** 1.6Kw, 3 phase 230-400v, 2 speed operation. 470 rpm. Max Flow 10500 L/h, max head 12M.

**GR MAJOR 60 –** 0.9Kw, 3 phase 230-400v, 2 speed operation. 235 rpm. Max Flow 5100 L/h, max head 8M.

**GR MAJOR 60 –** 2.2Kw, 3 phase 230-400v, 2 speed operation. 700 rpm. Max Flow 15000 L/h, max head 16M.

**GR MAJOR 60 –** 1.5Kw, 3 phase 230-400v, 2 speed operation. 350 rpm. Max Flow 7800 L/h, max head 12M.

**GR MAXI 80 -** 4Kw, 3 phase 230-400v, single speed operation. 470 rpm. Max Flow 34200 L/h, max head 16M.

**GR MAXI 80 -** 4Kw, 3 phase 230-400v, single speed operation. 600 rpm. Max Flow 41400 L/h, max head 16M.