**Liverani Flexible Impeller Pump RID Model Numbers.**

**RID MINOR 40 -** 1.5Kw, three phase 230-400v, single speed operation. 350 rpm. Max Flow 2500 L/h, max head 16M.

**RID MINOR 40 -** 1.5Kw, three phase 230-400v, single speed operation. 700 rpm. Max Flow 4700 L/h, max head 20M.

**RID MINOR 40 –** 2.2Kw, three phase 230-400v, 2 speed operation. 700 rpm. Max Flow 4700 L/h, max head 20M.

**RID MINOR 40 -** 1.5Kw, three phase 230-400v, 2 speed operation. 350 rpm. Max Flow 2500 L/h, max head 16M.

**RID MAJOR 60 –** 2.2Kw, three phase 230-400v, single speed operation. 235 rpm. Max Flow 5100 L/h, max head 4M.

**RID MAJOR 60 -** 2.2Kw, three phase 230-400v, single speed operation. 350 rpm. Max Flow 7800 L/h, max head 12M.

**RID MAJOR 60 -** 2.2Kw, three phase 230-400v, single speed operation. 470 rpm. Max Flow 10500 L/h, max head 12M.

**RID MAJOR 60 -**2.2Kw, three phase 230-400v, single speed operation. 700 rpm. Max Flow 15000 L/h, max head 16M.

**RID MAJOR 60 -** 2.2Kw, three phase 230-400v, 2 speed operation. 470 rpm. Max Flow 10500 L/h, max head 12M.

**RID MAJOR 60 –** 1.5Kw, three phase 230-400v, 2 speed operation. 235 rpm. Max Flow 5100 L/h, max head 4M.

**RID MAJOR 60 -** 2.2Kw, three phase 230-400v, 2 speed operation. 700 rpm. Max Flow 15000 L/h, max head 16M.

**RID MAJOR 60 -** 2.2Kw, three phase 230-400v, 2 speed operation. 350 rpm. Max Flow 7800 L/h, max head 12M.

**RID MAXI 80 –** 4Kw, three phase 230-400v, single speed operation. 235 rpm. Max Flow 18000 L/h, max head 12M.

**RID MAXI 80 -** 4Kw, three phase 230-400v, single speed operation. 300 rpm. Max Flow 22200 L/h, max head 12M.

**RID MAXI 80 -** 4Kw, three phase 230-400v, single speed operation. 470 rpm. Max Flow 34200 L/h, max head 16M.

**RID MAXI 80 -** 4Kw, three phase 230-400v, single speed operation. 600 rpm. Max Flow 41400 L/h, max head 16M.

**RID MAXI 80 –** 4.5Kw, three phase 230-400v, 2 speed operation. 470 rpm. Max Flow 34200 L/h, max head 16M.

**RID MAXI 80 –** 3.3Kw, three phase 230-400v, 2 speed operation. 235 rpm. Max Flow 18000 L/h, max head 12M.

**RID MAXI 80 -** 4.5Kw, three phase 230-400v, 2 speed operation. 600 rpm. Max Flow 41400 L/h, max head 16M.

**RID MAXI 80 –** 3.3Kw, three phase 230-400v, 2 speed operation. 300 rpm. Max Flow 22200 L/h, max head 12M.

**RID MAXI Double 2Q –** 5.5Kw, three phase 230-400v, single speed operation. 470 rpm. Max Flow 65000 L/h, max head 18M.

**RID MAXI Double 2Q -** 5.5Kw, three phase 230-400v, 2 speed operation. 470 rpm. Max Flow 65000 L/h, max head 18M.

**RID MAXI Double 2Q -** 3Kw, three phase 230-400v, 2 speed operation. 235 rpm. Max Flow 33000 L/h, max head 16M.

**RID MAXI Double 2H –** 5.5Kw, three phase 230-400v, single speed operation. 470 rpm. Max Flow 35000 L/h, max head 32M.

**RID MAXI Double 2H -** 5.5Kw, three phase 230-400v, 2 speed operation. 470 rpm. Max Flow 35000 L/h, max head 32M.

**RID MAXI Double 2H -** 3Kw, three phase 230-400v, 2 speed operation. 235 rpm. Max Flow 18500 L/h, max head 24M.