**Liverani Side Channel Pump EP Model Numbers.**

**EPH 20 –** Bronze. 2800rpm, 0.22 Kw, single phase 230v. ¾” BSP M inlet/outlet. Max flow 20 L/min. Max head 12M. With handle, on-off/reverse rocker switch, 1.5M cable and plug.

**EPH 25 –** Bronze. 2800rpm, 0.45 Kw, single phase 230v. 1” BSP M inlet/outlet. Max flow 50 L/min. Max head 15M. With handle, on-off/reverse rocker switch, 1.5M cable and plug.

**EP 20 T –** Bronze. 3000rpm, 0.45 Kw, direct current 12v/36A. ¾” BSP M inlet/outlet. Max flow 27 L/min. Max head 18M. With handle and terminal board connection.

**EP 20 T –** Bronze. 3000rpm, 0.45 Kw, direct current 24v/22A. ¾” BSP M inlet/outlet. Max flow 27 L/min. Max head 18M. With handle and terminal board connection.

**EP 20 –** Bronze. 2000rpm, 0.33 Kw, direct current 12v/26A. ¾” BSP M inlet/outlet. Max flow 18 L/min. Max head 5M. With handle and terminal board connection.

**EP 20 –** Bronze. 2000rpm, 0.33 Kw, direct current 24v/14A. ¾” BSP M inlet/outlet. Max flow 18 L/min. Max head 5M. With handle and terminal board connection.

**EP 20 –** Bronze. 2800rpm, 0.22 Kw, single phase, 230v. ¾” BSP M inlet/outlet. Max flow 20 L/min. Max head 12M. With handle, on-off/reverse rotary switch and 6M cable.

**EP 20 –** Bronze. 2800rpm, 0.26 Kw, three phase, 230-400v. ¾” BSP M inlet/outlet. Max flow 20 L/min. Max head 12M. With handle, on-off/reverse rotary switch and 6M cable.

**EP 20 –** Bronze. 2800rpm, 0.26 Kw, three phase, 230-400v. ¾” BSP M inlet/outlet. Max flow 20 L/min. Max head 12M. With handle and terminal board connection.

**EP 25 –** Bronze. 2000rpm, 0.45 Kw, direct current 12v/38A. 1” BSP M inlet/outlet. Max flow 37 L/min. Max head 10M. With handle and terminal board connection.

**EP 25 –** Bronze. 2000rpm, 0.45 Kw, direct current 24v/22A. 1” BSP M inlet/outlet. Max flow 37 L/min. Max head 10M. With handle and terminal board connection.

**EP 25 –** Bronze. 2800rpm, 0.45 Kw, single phase, 230v. 1” BSP M inlet/outlet. Max flow 50 L/min. Max head 15M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 25 –** Bronze. 2800rpm, 0.56 Kw, three phase, 230-400v. 1” BSP M inlet/outlet. Max flow 50 L/min. Max head 15M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 25 –** Bronze. 2800rpm, 0.56 Kw, three phase, 230-400v. 1” BSP M inlet/outlet. Max flow 50 L/min. Max head 15M. Terminal board connection. Handle on request.

**EP 30 –** Bronze. 1400rpm, 0.60 Kw, direct current 12v/28A. 1 ¼” BSP M inlet/outlet. Max flow 60 L/min. Max head 15M. With handle and terminal board connection.

**EP 30 –** Bronze. 1400rpm, 0.75 Kw, single phase, 230v. 1 ¼” BSP M inlet/outlet. Max flow 60 L/min. Max head 15M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 30 –** Bronze. 1400rpm, 0.75 Kw, three phase, 230-400v. 1 ¼” BSP M inlet/outlet. Max flow 60 L/min. Max head 15M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 30 –** Bronze. 1400rpm, 0.75 Kw, three phase, 230-400v. 1 ¼” BSP M inlet/outlet. Max flow 60 L/min. Max head 15M. Terminal board connection. Handle on request.

**EP 40 –** Bronze. 1400rpm, 1.12 Kw, direct current 24v/45A. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 18M. With handle and terminal board connection.

**EP 40 –** Bronze. 1400rpm, 0.75 Kw, single phase, 230v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 18M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 40 –** Bronze. 1400rpm, 1.12 Kw, single phase, 230v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 18M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 40 –** Bronze. 1400rpm, 0.75 Kw, three phase, 230-400v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 18M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 40 –** Bronze. 1400rpm, 1.12 Kw, three phase, 230-400v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 18M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP 40 –** Bronze. 1400rpm, 0.75 Kw, three phase, 230-400v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 18M. Terminal board connection. Handle on request.

**EP 50 –** Bronze. 1400rpm, 1.5 Kw, direct current 24v/95A. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. Terminal board connection.

**EP 50 –** Bronze. 1400rpm, 1.86 Kw, single phase 230v. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. On-off/reverse rotary switch and 6M cable.

**EP 50 –** Bronze. 1400rpm, 1.86 Kw, three phase 230-400v. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. On-off/reverse rotary switch and 6M cable.

**EP 50 –** Bronze. 1400rpm, 1.86 Kw, three phase 230-400v. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. Terminal board connection.

**EP 70 –** Bronze. 1400rpm, 5.5 Kw, three phase 230-400v. 2 ½” BSP F inlet/outlet. Max flow 460 L/min. Max head 30M. Terminal board connection.

**EP 70 –** Bronze. 1400rpm, 7.5 Kw, three phase 230-400v. 2 ½” BSP F inlet/outlet. Max flow 460 L/min. Max head 30M. Terminal board connection.

**EPH NEOS ¾” –** Stainless steel AISI 316. 2800rpm, 0.22 Kw, single phase 230v. ¾” BSP M inlet/outlet. Max flow 23 L/min. Max head 20M. On-off/reverse rocker switch, 1.5M cable and plug. Handle on request.

**EP NEOS ¾” T –** Stainless steel AISI 316. 3000rpm, 0.45 Kw, direct current 12v/36A. ¾” BSP M inlet/outlet. Max flow 30 L/min. Max head 20M. With handle and terminal board connection.

**EP NEOS ¾” T –** Stainless steel AISI 316. 3000rpm, 0.45 Kw, direct current 24v/22A. ¾” BSP M inlet/outlet. Max flow 30 L/min. Max head 20M. With handle and terminal board connection.

**EP NEOS ¾” –** Stainless steel AISI 316. 2000rpm, 0.33 Kw, direct current 12v/26A. ¾” BSP M inlet/outlet. Max flow 18 L/min. Max head 10M. With handle and terminal board connection.

**EP NEOS ¾” –** Stainless steel AISI 316. 2000rpm, 0.33 Kw, direct current 24v/14A. ¾” BSP M inlet/outlet. Max flow 18 L/min. Max head 10M. With handle and terminal board connection.

**EP NEOS ¾” –** Stainless steel AISI 316. 2800rpm, 0.22 Kw, single phase 230v. ¾” BSP M inlet/outlet. Max flow 23 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP NEOS ¾” –** Stainless steel AISI 316. 2800rpm, 0.26 Kw, three phase 230-400v. ¾” BSP M inlet/outlet. Max flow 23 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP NEOS ¾” –** Stainless steel AISI 316. 2800rpm, 0.26 Kw, three phase 230-400v. ¾” BSP M inlet/outlet. Max flow 23 L/min. Max head 20M. Terminal board connection. Handle on request.

**EP JUNIOR 1” ¼ -** Stainless steel AISI 316. 2000rpm, 0.37 Kw, direct current 12v/32A. 1 ¼” BSP M inlet/outlet. Max flow 25 L/min. Max head 5M. With handle and terminal board connection.

**EP JUNIOR 1” ¼ -** Stainless steel AISI 316. 2000rpm, 0.37 Kw, direct current 24v/20A. 1 ¼” BSP M inlet/outlet. Max flow 25 L/min. Max head 5M. With handle and terminal board connection.

**EP JUNIOR 1” ¼ -** Stainless steel AISI 316. 2800rpm, 0.45 Kw, single phase 230v. 1 ¼” BSP M inlet/outlet. Max flow 47 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP JUNIOR 1” ¼ -** Stainless steel AISI 316. 2800rpm, 0.56 Kw, three phase 230-400v. 1 ¼” BSP M inlet/outlet. Max flow 47 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP JUNIOR 1” ¼ -** Stainless steel AISI 316. 2800rpm, 0.56 Kw, three phase 230-400v. 1 ¼” BSP M inlet/outlet. Max flow 47 L/min. Max head 20M. Terminal board connection. Handle on request.

**EP SENIOR 1” ½ -** Stainless steel AISI 316. 1400rpm, 1.12 Kw, direct current 24v/45A. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 20M. With handle and terminal board connection.

**EP SENIOR 1” ½ -** Stainless steel AISI 316. 1400rpm, 0.75 Kw, single phase 230v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP SENIOR 1” ½ -** Stainless steel AISI 316. 1400rpm, 1.12 Kw, single phase 230v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP SENIOR 1” ½ -** Stainless steel AISI 316. 1400rpm, 0.75 Kw, three phase 230-400v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP SENIOR 1” ½ -** Stainless steel AISI 316. 1400rpm, 1.12 Kw, three phase 230-400v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 20M. On-off/reverse rotary switch and 6M cable. Handle on request.

**EP SENIOR 1” ½ -** Stainless steel AISI 316. 1400rpm, 1.12 Kw, three phase 230-400v. 1 ½” BSP M inlet/outlet. Max flow 110 L/min. Max head 20M. Terminal board connection. Handle on request.

**EP MASTER 2” –** Stainless steel AISI 316. 1400rpm, 1.5 Kw, direct current 24v/95A. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. Terminal board connection.

**EP MASTER 2” –** Stainless steel AISI 316. 1400rpm, 1.86 Kw, single phase 230v. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. On-off/reverse rotary switch and 6M cable.

**EP MASTER 2” –** Stainless steel AISI 316. 1400rpm, 1.86 Kw, three phase 230-400v. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. On-off/reverse rotary switch and 6M cable.

**EP MASTER 2” –** Stainless steel AISI 316. 1400rpm, 1.86 Kw, three phase 230-400v. 2” BSP M inlet/outlet. Max flow 210 L/min. Max head 22M. Terminal board connection.

**EP 70 Inox -** Stainless steel AISI 316. 1400rpm, 5.5 Kw, three phase 230-400v. DN65 inlet/outlet. Max flow 460 L/min. Max head 30M. Terminal board connection.

**EP 70 Inox -** Stainless steel AISI 316. 1400rpm, 7.5 Kw, three phase 230-400v. DN65 inlet/outlet. Max flow 460 L/min. Max head 30M. Terminal board connection.