**Liverani Side Channel Pump GRADPE Model Numbers.**

**GRADPE NAUTIC 30 Bronzo –** 1 ¼” BSP-M inlet/outlet. Bronze with base. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 60 L/min. Max head 10M.

**GRADPE NAUTIC 30 Bronzo -** 1 ¼” BSP-M inlet/outlet. Bronze with trolley. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 60 L/min. Max head 10M.

**GRADPE NAUTIC 40 Bronzo –** 1 ½” BSP-M inlet/outlet. Bronze with base. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 110 L/min. Max head 18M.

**GRADPE NAUTIC 40 Bronzo -** 1 ½” BSP-M inlet/outlet. Bronze with trolley. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 110 L/min. Max head 18M.

**GRADPE NAUTIC 50 Bronzo –** 2” BSP-M inlet/outlet. Bronze with base. 1400 rpm, 1.5Kw, three phase 230-400v. Max flow 210 L/min. Max head 22M.

**GRADPE NAUTIC 50 Bronzo –** 2” BSP-M inlet/outlet. Bronze with trolley. 1400 rpm, 1.5Kw, three phase 230-400v. Max flow 210 L/min. Max head 22M.

**GRADPE NAUTIC 70 Bronzo –** 2 ½” BSP-F inlet/outlet. Bronze with base. 1400 rpm, 5.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.

**GRADPE NAUTIC 70 Bronzo -** 2 ½” BSP-F inlet/outlet. Bronze with trolley. 1400 rpm, 5.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.

**GRADPE NAUTIC 70 Bronzo –** 2 ½” BSP-F inlet/outlet. Bronze with base. 1400 rpm, 7.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.

**GRADPE NAUTIC 70 Bronzo –** 2 ½” BSP-F inlet/outlet. Bronze with trolley. 1400 rpm, 7.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.

**GRADPE SPECIAL 30 Bronzo –** 1 ¼” BSP-M inlet/outlet. Bronze with base. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 60 L/min. Max head 10M.

**GRADPE SPECIAL 30 Bronzo -** 1 ¼” BSP-M inlet/outlet. Bronze with trolley. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 60 L/min. Max head 10M.

**GRADPE SPECIAL 40 Bronzo –** 1 ½” BSP-M inlet/outlet. Bronze with base. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 110 L/min. Max head 18M.

**GRADPE SPECIAL 40 Bronzo -** 1 ½” BSP-M inlet/outlet. Bronze with trolley. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 110 L/min. Max head 18M.

**GRADPE SPECIAL 50 Bronzo –** 2” BSP-M inlet/outlet. Bronze with base. 1400 rpm, 1.5Kw, three phase 230-400v. Max flow 210 L/min. Max head 22M.

**GRADPE SPECIAL 50 Bronzo -** 2” BSP-M inlet/outlet. Bronze with trolley. 1400 rpm, 1.5Kw, three phase 230-400v. Max flow 210 L/min. Max head 22M.

**GRADPE SPECIAL SENIOR 1” ½ Inox –** 1 ½” BSP-M inlet/outlet. Stainless steel with base. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 110 L/min. Max head 18M.

**GRADPE SPECIAL SENIOR 1” ½ Inox –** 1 ½” BSP-M inlet/outlet. Stainless steel with trolley. 1400 rpm, 0.75Kw, three phase 230-400v. Max flow 110 L/min. Max head 18M.

**GRADPE SPECIAL MASTER 2” Inox –** 2” BSP-M inlet/outlet. Stainless steel with base. 1400 rpm, 1.5Kw, three phase 230-400v. Max flow 210 L/min. Max head 22M.

**GRADPE SPECIAL MASTER 2” Inox –** 2” BSP-M inlet/outlet. Stainless steel with trolley. 1400 rpm, 1.5Kw, three phase 230-400v. Max flow 210 L/min. Max head 22M.

**GRADPE NAUTIC 70 Inox –** 2 ½” BSP-M inlet/outlet. Stainless steel with base. 1400 rpm, 5.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.

**GRADPE NAUTIC 70 Inox -** 2 ½” BSP-M inlet/outlet. Stainless steel with trolley. 1400 rpm, 5.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.

**GRADPE NAUTIC 70 Inox –** 2 ½” BSP-M inlet/outlet. Stainless steel with base. 1400 rpm, 7.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.

**GRADPE NAUTIC 70 Inox -** 2 ½” BSP-M inlet/outlet. Stainless steel with trolley. 1400 rpm, 7.5Kw, three phase 230-400v. Max flow 460 L/min. Max head 30M.