**Liverani Flexible Impeller Pump S/P Model Numbers.**

**S/P MINOR 40 –** Bare shaft. Max 900 rpm. Max Flow 6200 L/h, max head 24M.

**S/P MAJOR 60 –** Bare shaft. Max 900 rpm. Max Flow 19560 L/h, max head 16M.

**S/P MAXI 80 -** Bare shaft. Max 600 rpm. Max Flow 41400 L/h, max head 16M.