**Liverani Flexible Impeller Pump VA Model Numbers.**

**VA MINOR 40 –** 1.5Kw, three phase 230-400v, 50Hz. 900 rpm. Max flow 6200 l/h, max head 24M.

**VA MAJOR 60 –** 1.87Kw, three phase 230-400v, 50Hz. 900 rpm. Max flow 19560 l/h, max head 16M.

**VA MAXI 80 –** 4Kw, three phase 230-400v, 50Hz. 600 rpm. Max flow 41400 l/h, max head 16M.